**Turdalin Nurassyl LAB1**

**2.5.5**

**Part 1**

1. How many FE interfaces does the switch have? – 24
2. GE – 2
3. vty – (0, 4) and (5, 15)
4. which command will display the current contents of NVRAM - show startup-config
5. startup-config is not present – because config wasn’t saved before/  
    **Part 2**
6. for enable secret - 5 $1$mERr$ILwq/b7kc.7X/ejA4Aosn0
7. differently from what we configured – because it was encrypted
8. If you configure more passwords on the switch, will they be displayed… - If I configure any more passwords, they will be displayed as plain text. This is because I serviced the other passwords to be encrypted. If I wanted passwords to be re-encrypted, I would need to re-enter the "Switch(config)#service password-encryption" command.  
    **Part 3**
9. Banner will display when we first time connect to router and we can see this in configuration
10. MOTD Banner – users will be updated on various activities, and it can also be used to warn against un-authorized access.
11. Short form - copy run start

**Result:**

Изображение выглядит как текст, снимок экрана, компьютер, внутренний

Автоматически созданное описание

