**Turdalin Nurassyl LAB1**

**2.7.6**

**Part 1**

1. We can verify passwords – 1) from show run 2) write them when connecting to console
2. Copy run start from priv. EXEC mode(S1#)  
   **Part 2**
3. Ping 1.253 – wasn’t successful because we didn’t configured such device with such IP, in our case these are switches.  
   **Part 3**
4. If this is the case, why would we configure it with an IP address? - To connect remotely to a switch, you need to assign an IP address to it. The default configuration on the switch is to have the management of the switch controlled through VLAN 1.
5. No shotdown - The no shutdown command administratively places the interface in an active state.

**Result:**

Изображение выглядит как текст, снимок экрана, компьютер, внутренний

Автоматически созданное описание

