**Turdalin Nurassyl LAB3**

**4.7.1**

1. Which management ports are available – **AUX, console**
2. **WAN interface is available. There are 2 of them. And also 2 GE interfaces**
3. How many physical interfaces are listed? – **4**
4. Default bandwidth of GE – **10^6 Kbits**
5. Default bandwidth of Serial – **1544 Kbits**
6. How many expansion slots are available to add additional modules to the East router? – **1**
7. On Switch 2 - **5 slots**
8. Module for East router – **HWIC-4ESW module**
9. **4** hosts can be connected
10. Module for Switch3 – **PT-SWITCH-NM-1FGE**
11. Into which slot was it inserted – **GE5/1**

**RESULT:**



