**Turdalin Nurassyl LAB5**

**10.1.4**

**PART 1**

1. Hostname: Router  
   FE: 3  
   GE: 2  
   SI: 2  
   vty: 0-4
2. Because we change anything
3. Show run
4. Banners: to say some information for unauthorized users
5. Secret will be required, because it will always override password.
6. After encryption they all will be encrypted
7. Wr mem or copy run start
8. Show run
9. 3 flashes.
10. With .bin format
11. It’s larger than others

Изображение выглядит как текст

Автоматически созданное описание