

**Turdalin Nurassyl LAB5**

**10.4.4**

**PART 1**

1. We didn’t configure Router till the end
2. After configuration it was successful
3. G0/0/0 and G0/0/1 on 4221 Router
4. Operational status: GE0/0/1 is up, line protocol is up
5. IP: 192.168.1.1/24
6. No shutdown, shutdown (on/off)
7. Cause of not correct IP addresses and default gateways on PC’s will be different, it won’t ping to each other.

****

****