**Turdalin Nurassyl LAB8**

**14.8.1**

1. Multiplex
2. Type of protocol
3. First of all there works TCP protocol to make everything, after that only HTTP appears.
4. TCP
5. SRC – 1026, DEST – 80, SEQ, ACK NUM – 1, 1
6.  ACK, PSH
7. SRC and DEST reversed, ACK, SYN
8. Now they reversed again, ACK, PSH
9. SRC – 1026, DEST – 21, SEQ AND ACK – 0,0
10. Message: Welcome to PT FTP server
11. Layer 4 – UDP
12. Reliable – No
13. SRC – 1026, DEST – 53
14. They reversed
15. DNS, 192.168.1.254
16. Email uses – TCP